| FST WebDemo |

Back to index Next Previous

To display FST operands a special tag <FSTCI> can be used. The FST web server will replace this tag with the result of the CI command. Some examples:

    The value of inputword 0: <FSTCI dew0>
    The value of inputword 1: <FSTCI dew1>
    The value of outputword 0: <FSTCI daw0>
    The value of outputword 1: <FSTCI daw1>
    The value of flagword 0: <FSTCI dmw0>
    The value of flagword 1: <FSTCI dmw1>
Result:
|  | The value of inputword 0: The value of inputword 1: The value of outputword 0: The value of outputword 1: The value of flagword 0: The value of flagword 1:

The syntax that must be used is the same as using CI commands, see the FST manual for more details.

Comments / remarks: i-sales@beck-ipc.com | Last modified: 2000.05.09